

This directory contains files that implement a server for the TAO
Notification Service.  In addition, it contains files that run the TAO
Notification Service as a Windows NT Service.  Both of these services
are described below.

How to Run the TAO Notification Service
=======================================

The tao_cosnotification executable starts up a Notification Service factory
and registers it with the Naming Service under the name
"NotifyEventChannelFactory"

Command line arguments:
----------------------
"-?"                    : shows the options.

"-Factory factory_name" : Uses the <factory_name> as the default name for the
                          Channel Factory
                          The default is "NotifyEventChannelFactory".

"-Boot"                 : Flag asking that the <factory_name> be registered
                          in the IOR table.
                          The option is disabled by default.
                          See the "Using the Boot option" section below.

"-NameSvc"              : Registers the Factory and if specified, an Event
                          Channel with the Naming Service.
                          if this option is used, a Naming Service must
                          be accessible.
                          This option is enabled by default.

"-NoNameSvc"            : Asks to skip any registration with the
                          Naming Service.
                          This option is disabled by default.

"-IORoutput file_name"  : The IOR is output to the file <file_name>.
                          By default, the IOR is printed out.

"-Channel"              : If this option is specified, a EventChannel is
                          created and registered with the Naming Service.
                          This option is disabled by default. This option can
                          be specified multiple times, each option will result
                          in a created and registered EventChannel


"-ChannelName channel_name" : Specifies the <channel_name> to register with the
                              Naming Service.
                              The default is "NotifyEventChannel".

"-RunThreads nthreads"   : Number of threads to run the
                           ORB::run method.

"-UseSeparateDispatchingORB 1|0"
                            : Indicates whether the service should create and
                              and use a separate ORB dedicated to dispatching of
                              events.

"-ShutdownORB 1|0" : Indicates that we have to shutdown the default ORB,
                     1 by default

"-ShutdownDispatchingORB 1|0" : Indicates that we have to shutdown the
                                dispatching ORB, 1 by default

"-Timeout msec" : Applies a relative round-trip timeout of msec microseconds
                  to the main ORB and, if -UseSeparateDispatchingORB 1 is
                  specified, to the dispatching ORB.  This requires the
                  'corba_messaging' MPC feature during building of the
                  tao_cosnotification, which is on by default.

"-LoggingInterval seconds" : Sets up a logging interval timer for the ORB's
                             reactor.  This is required to use the ACE
                             Logging Service features such as file sizing
                             and rotation.  See the example below.

!! The -Notify_TPReactor option is deprecated!! use the -ORBRunThreads
option instead.

"-Notify_TPReactor [threads]": Tells the Notify Service that the ORB
                               will use a TP reactor and specifies the
                               number of worker threads to utilize.


Note that the svc.conf file must instruct the ORB to use a TP reactor
e.g. static Resource_Factory "-ORBReactorType tp -ORBReactorMaskSignals 0"
Please look up the ORB configuration options to get more information
on this.

Running the Service:
-------------------
1. Start the Naming Service from

$TAO_ROOT/orbsvcs/Naming_Service/Naming_Service -m 1

if you are using the "-NameSvc" options.

2.Start the Notify_Service from this directory. You should see a message saying
  that the service has been started.

   Note:
   ====
   By default, the Naming Service disables multicast discovery.
   The "-m 1" option enables the Naming Service to be resolved via
   multicast.

   If you do not wish to do this, then use the
   -ORBInitRef option in which case the Naming Service should be started
   as:

   $TAO_ROOT/orbsvcs/Naming_Service/Naming_Service -o naming.ior

   and the Notify_Service as

   $ tao_cosnotification -ORBInitRef NameService=file://naming.ior

Using the Boot option:
----------------------
an example on how to locate the Notify Factory without the Naming Service -

./tao_cosnotification -Boot -NoNameSvc -d -ORBobjrefstyle url -ORBEndPoint "iiop://flamenco.cs:9999"

The Factory object reference is not registered with the Naming Service.
"-Boot" binds the Factory object reference with "NotifyEventChannelFactory" in
the IOR table.
See the $TAO_ROOT/docs/Options.html for details on "-ORBEndPoint"

A client program can obtain the factory object reference in the following
manner:
./client -ORBInitRef "NotifyEventChannelFactory=corbaloc:iiop:flamenco.cs:9999/NotifyEventChannelFactory"

Note that the client uses:
 resolve_initial_references ("NotifyEventChannelFactory");
to obtain the object reference.

Using the ACE Logging Service:
------------------------------

Start the tao_cosnotification executable with the debug options desired and
the -LoggingInterval option:

./tao_cosnotification -ORBDebugLevel 10 -ORBVerboseLogging 1 -ORBSvcConf ns.conf -LoggingInterval 5

Configure the logging service in the ns.conf file:
dynamic Logging_Strategy Service_Object * ACE:_make_ACE_Logging_Strategy() "-s NS -f OSTREAM -t 0 "



The svc.conf options:
----------------------

The "TAO_CosNotify_Service" service object accepts the following options:

"-AllocateTaskperProxy"              : Allocate worker tasks per proxy
                                       *see footnote below for explanation*

"-AllowReconnect"                    : Allows consumers and suppliers to
                                       reconnect to existing proxies.

"-AsynchUpdates"                     : Send subscription and publication
                                       updates asynchronously.

"-DefaultConsumerAdminFilterOp [op]" : Sets the default consumer admin filter
                                       operator. op can be either "OR" or
                                       "AND". The default is "OR" to be
                                       consistent with older releases of TAO.

"-DefaultSupplierAdminFilterOp [op]" : Sets the default supplier admin filter
                                       operator. op can be either "OR" or
                                       "AND". The default is "OR" to be
                                       consistent with older releases of TAO.

"-DispatchingThreads [thread_count]" : Enables MT dispatching with the
                                       specified number of threads. This
                                       option supercedes the deprecated
                                       ListenerThreads, MTListenerEval and
                                       MTDispatching options. Note that
                                       "AllocateTaskperProxy" affects how this
                                       value is applied.

"-NoUpdates"                         : Globally disables subscription and
                                       publication updates.

"-ValidateClient"                    : Creates a thread that periodically
                                       walks the topology tree visiting each
                                       proxy and checking the liviness of
                                       the peer. A peer which had ordinary
                                       activity within the validation time
                                       period is considered alive. Otherwise
                                       the peer's _non_existent() operation
                                       is invoked. If this fails the proxy's
                                       disconnect operation is invoked.

"-ValidateClientDelay [sec]"         : Specifies the initial delay from the
                                       start of the validator task until the
                                       first pass through the topology. If
                                       left at the default value of 0, the
                                       validator taks will start immediately.
                                       A long delay is useful when the Notify
                                       service restarts after a shutdown and
                                       has to repopulate its topology from a
                                       persistent store, which takes time.

"-ValidateClientInterval [sec]"      : Specifies how frequently after the
                                       first pass to revisit the topology
                                       to further validate clients. The
                                       default value of 0 means validation
                                       will only happen once.

"-SourceThreads [thread_count]"      : Specifies the number of threads for each
                                       supplier admin or proxy consumer. See
                                       the note below for details about thread
                                       assignments. This option supercedes the
                                       deprecated LookupThreads, MTSourceEval,
                                       and MTLookup options.

All other options are deprecated and should not be used.

e.g. svc.conf
static TAO_CosNotify_Service "-DispatchingThreads 2"

This means that we want to enable event dispatching with 2 threads.

----------------------------------------------------------------
What does the "-AllocateTaskperProxy" option do?

A Task here implies a thread pool that performs a fixed work in the
Notify Service. e.g. When you specify "-DispatchingThreads 1" this
means there is 1 thread to perform the event dispatching to consumers
IRRESPECTIVE OF THE NUMBER OF PROXY SUPPLIERS. It also means that
events destined for each consumer will be queued to a buffer for that
consumer.  Therefore, you can also think of this option as Enable
Consumer-side Buffering of Events.

This is the default case.

When you specify "-AllocateTaskperProxy" it asks notify to create a
dispatching task with the specified thread pool size PER PROXY
SUPPLIER.  So if you use this option and connect 50 consumers with 1
thread for the dispatching task you will have created 50 dispatching
threads! so use this option with care and you might not need it in
most cases.

Why have this feature in the first place?  The intent is to allow the
software architect of a Notify based system, fine control over where
and how much thread resources are deployed.  e.g. a channel could have
2 proxy suppliers - the first one delivers an important event in huge
quantities.  A dedicated thread pool to this proxy will ensure better
throughput to it's consumers. (Eventually I want to be able to set the
thread pool size via a QoS property)

Similarly "-SourceThreads 2" specifies a thread pool for use by the
supplier-side processing. This enables Buffering on the Supplier-side,
with the thread pool being used to process supplier side filters and
push the events to the Consumer side.

How to use the NT_Notify_Service
================================

To set the options for the TAO Notification Service, go to the Services
icon in the Settings group under the start menu (start menu ->
settings -> services).  There, highlight the NT_Notify_Service, which
is the name used by the Notification Service when it is registered.
After it's highlighted, you should see at the bottom of the dialog box
an area to specify options.  Just enter the options you wish in that
edit box and everything should just work.  However, some options, such
as -ORBDebugLevel, won't work since an NT service can't write output
to standard out.

1. Syntax

        % tao_nt_cosnotification [-i n]
                                 [-c [args]]
                                 [-r]
                                 [-s]
                                 [-k]
                                 [-t n]
                                 [-d]

2. Optional Command-line Arguments

        -i [n]
                Install this program as an NT service, with specified startup mode

        -c [args]
                Query or supply command line arguments for NT service.

        -r
                Remove this program from the Service Manager
        -s
                Start the service

        -k
                Kill the service

        -t n
                Set startup mode for an existing service

        -d
                Debug; run as a regular application

3. Usage

        To see different stages of an NT service application, you have
        to run the program several times, with different options.
        Please note: run with only one option at a time. Only the
        Administrator can run commands that modify state such as the -i
        or -c options.

        a. First, you must initialize the service in the NT SCM
           database.  Run tao_nt_cosnotification with -i [n], where n is a
           number from 1 to 4, corresponding to these startup options:

           // Start Type (from WinNT.h)
           //
           #define SERVICE_SYSTEM_START    0x00000001
           #define SERVICE_AUTO_START      0x00000002
           #define SERVICE_DEMAND_START    0x00000003
           #define SERVICE_DISABLED        0x00000004

           If only -i is specified, SERVICE_DEMAND_START is default option.
           This option may only be run as Administrator.

        b. For System or Auto start modes, or even Demand start and using the
           -s option to start, any command line options, such as endpoint
           specification or IOR publication, must be stored in the Windows
           registry. Use tao_nt_cosnotification -c with no additional arguments to
           see the current command line setting. Use tao_nt_cosnotification -c "args"
           to provide a new command line for the registered name service. Be
           sure to quote the args string. For example:

           tao_nt_cosnotification -c "-ORBListenEndpoints iiop://%computername%:2809"

           will yield:
           tao_nt_cosnotification -c
           -ORBListenEndpoints iiop://VIRTWIND:2809

           Notice the environment variable used in the argument string was
           expanded.

        c. Now you are ready to run the actual service. Run
           tao_nt_cosnotification -s.

        d. To stop service execution, run tao_nt_cosnotification -k.

        c. To remove the service from the Service Control Manager
           database, run tao_nt_cosnotification -r.

        In addition, once you have initialized this service (by using
        the -i option) you can change its startup type to one of the
        other values above.  To do this, run tao_nt_cosnotification -t n, where
        n is a number corresponding to one of the startup modes listed above.

        In order to debug the service's execution itself, use the -d
        option.
