Main Page Namespace List Class Hierarchy Alphabetical List Compound List File List Namespace Members Compound Members File Members

# TAO_AV Compound List

Here are the classes, structs, unions and interfaces with brief descriptions:

- AVStreams::alreadyConnected (No description available)
- AV_Null_MediaCtrl (No description available)
- POA_AVStreams::Basic_StreamCtrl (No description available)
- AVStreams::Basic_StreamCtrl (Base class for StreamCtrl, implements basic stream start and stop functionality)
- TAO_AV_RTP::bvchdr (No description available)
- TAO_AV_RTP::cellbhdr (No description available)
- flowProtocol::credit (No description available)
- AVStreams::deviceQosMismatch (No description available)
- AVStreams::failedToConnect (No description available)
- AVStreams::failedToListen (No description available)
- POA_AVStreams::FDev (No description available)
- AVStreams::FDev (No description available)
- AVStreams::FEPMismatch (No description available)
- Fill_ACE_QoS (No description available)
- POA_AVStreams::FlowConnection (No description available)
- AVStreams::FlowConnection (No description available)
- POA_AVStreams::FlowConsumer (No description available)
- AVStreams::FlowConsumer (No description available)
- POA_AVStreams::FlowEndPoint (No description available)
- AVStreams::FlowEndPoint (No description available)
- POA_AVStreams::FlowProducer (No description available)
- AVStreams::FlowProducer (No description available)
- AVStreams::flowStatus (Used to store the status of a flow)
- AVStreams::formatMismatch (No description available)
- AVStreams::formatNotSupported (No description available)
- AVStreams::FPError (No description available)
- flowProtocol::fragment (No description available)
- flowProtocol::frame (No description available)
- flowProtocol::frameHeader (No description available)
- AVStreams::InvalidPosition (No description available)
- AVStreams::invalidSettings (No description available)
- TAO_AV_RTP::jpeghdr (No description available)
- POA_AVStreams::MCastConfigIf (No description available)
- AVStreams::MCastConfigIf (Interface for multicasting operations)
- POA_AVStreams::MediaControl (No description available)
- AVStreams::MediaControl (MediaControl interface is similar to ControlledStream interface in MSS. It can be inherited by flow endpoints or FlowConnection interfaces)
- MediaTimer (No description available)
- POA_AVStreams::MMDevice (No description available)
- AVStreams::MMDevice (Implements a factory to create Endpoints and VDevs)
- TAO_StreamCtrl::MMDevice_Map_Entry (No description available)
- MMDevice_Map_Hash_Key (No description available)
- POA_AVStreams::Negotiator (No description available)
- AVStreams::Negotiator (This interface is used to negotiate QoS between two stream endpoints)
- AVStreams::noSuchFlow (No description available)
- AVStreams::notConnected (No description available)
- AVStreams::notSupported (No description available)
- TAO_AV_RTCP::ntp64 (No description available)
- Null_MediaCtrl (No description available)
- TAO_AV_RTP::nvhdr (No description available)
- TAO_MCastConfigIf::Peer_Info (No description available)
- POA_Null_MediaCtrl (No description available)
- AVStreams::Position (No description available)
- AVStreams::MediaControl::PostionKeyNotSupported (No description available)
- AVStreams::PostionKeyNotSupported (No description available)
- AVStreams::PropertyException (No description available)
- AVStreams::CosPropertyService::PropertySet (No description available)
- AVStreams::protocolNotSupported (No description available)
- AVStreams::QoS (This structure represents QoS for a given type. E.g. {"video_qos", <"video_framerate", 26>, <"video_depth", 9>})
- AVStreams::QoSRequestFailed (No description available)
- TAO_AV_RTCP::rtcp_rr (No description available)
- TAO_AV_RTCP::rtcp_sr (No description available)
- TAO_AV_RTCP::rtcphdr (No description available)
- TAO_AV_RTP::rtphdr (No description available)
- flowProtocol::sequencedFrame (No description available)
- AVStreams::SFPStatus (This structure is defined for SFP1.0 Subsequent versions of the protocol may specify new structures)
- flowProtocol::specialFrame (No description available)
- flowProtocol::Start (No description available)
- flowProtocol::StartReply (No description available)
- POA_AVStreams::StreamCtrl (No description available)
- AVStreams::StreamCtrl (Implementation the A/V StreamCtrl class. this class is used to control the stream. It should be subclassed by applications that want to provide more control features)
- POA_AVStreams::StreamEndPoint (No description available)
- AVStreams::StreamEndPoint (No description available)
- AVStreams::StreamEndpoint (The Stream EndPoint. Used to implement one endpoint of a stream that implements the transport layer)
- POA_AVStreams::StreamEndPoint_A (No description available)
- AVStreams::StreamEndPoint_A (The "A" side of a streamendpoint)
- POA_AVStreams::StreamEndPoint_B (No description available)
- AVStreams::StreamEndPoint_B (The "B" side of a streamendpoint)
- AVStreams::streamOpDenied (No description available)
- AVStreams::streamOpFailed (No description available)
- TAO_AV_Acceptor (No description available)
- TAO_AV_Acceptor_Registry (No description available)
- TAO_AV_Base_Connector (No description available)
- TAO_AV_Callback (Callback class that the user will be implementing for receiving frames from the network and also for timer events)
- TAO_AV_Child_Process (Helper class for the child process created in TAO_AV_Endpoint_Process_Strategy)
- TAO_AV_Child_Process_A (Helper class for the child process created in TAO_AV_Child_Process)
- TAO_AV_Child_Process_B (Helper class for the child process created in TAO_AV_Child_Process)
- TAO_AV_Connector (No description available)
- TAO_AV_Connector_Registry (No description available)
- TAO_AV_Core (This class encapsulates access to the TAO AV Core's resources and its state)
- TAO_AV_Endpoint_Process_Strategy (No description available)
- TAO_AV_Endpoint_Process_Strategy_A (Process-based strategy to create "A" type endpoints)
- TAO_AV_Endpoint_Process_Strategy_B (Process-based strategy to create "B" type endpoints)
- TAO_AV_Endpoint_Reactive_Strategy (Reactive strategy base class)
- TAO_AV_Endpoint_Reactive_Strategy_A (Reactive strategy)
- TAO_AV_Endpoint_Reactive_Strategy_B (Reactive strategy)
- TAO_AV_Endpoint_Strategy (Process-based strategy for creating endpoints. Abstract base class)
- TAO_AV_Flow_Handler (No description available)
- TAO_AV_Flow_Protocol_Factory (No description available)
- TAO_AV_Flow_Protocol_Item (No description available)
- TAO_AV_frame_info (No description available)
- TAO_AV_Payload_Type_Policy (No description available)
- TAO_AV_Policy (No description available)
- TAO_AV_Protocol_Object (TAO_AV_Protocol_object for the RTP protocol)
- TAO_AV_QoS (Class for getting and setting the QoS characteristics of an AV Stream)
- TAO_AV_RTCP (Encapsulate the header format for the Real Time Control Protocol (RTCP))
- TAO_AV_RTCP_Callback (TAO_AV_Callback for RTCP protocol)
- TAO_AV_RTCP_Flow_Factory (No description available)
- TAO_AV_RTCP_Object (TAO_AV_Protocol_Object for RTCP protocol)
- TAO_AV_RTCP_Sdes (No description available)
- TAO_AV_RTCP_Sdes_Policy (No description available)
- TAO_AV_RTP (Encapsulate the Real Time Protocol (RTP) header format)
- TAO_AV_RTP_Flow_Factory (No description available)
- TAO_AV_RTP_Object (No description available)
- TAO_AV_RTP_State (Encapsulate the state of an RTP session)
- TAO_AV_SFP_Credit_Policy (No description available)
- TAO_AV_SFP_Factory (No description available)
- TAO_AV_Source (No description available)
- TAO_AV_SourceManager (No description available)
- TAO_AV_SSRC_Policy (No description available)
- TAO_AV_TCP_Acceptor (No description available)
- TAO_AV_TCP_Base_Acceptor (No description available)
- TAO_AV_TCP_Base_Connector (No description available)
- TAO_AV_TCP_Connector (No description available)
- TAO_AV_TCP_Factory (No description available)
- TAO_AV_TCP_Flow_Factory (No description available)
- TAO_AV_TCP_Flow_Handler (No description available)
- TAO_AV_TCP_Object (TAO_AV_Protocol_Object for Transmission Control Protocol (TCP))
- TAO_AV_TCP_Transport (A transport abstraction for socket streams. Uses the ACE_SOCK_Stream to send the data)
- TAO_AV_Transport (A Base class for the different transport protocols. All the different transports should derive and implement the open,close,send and recv methods)
- TAO_AV_Transport_Factory (No description available)
- TAO_AV_Transport_Item (No description available)
- TAO_AV_UDP_Acceptor (No description available)
- TAO_AV_UDP_Connector (No description available)
- TAO_AV_UDP_Factory (No description available)
- TAO_AV_UDP_Flow_Factory (No description available)
- TAO_AV_UDP_Flow_Handler (Flow Handler for UDP flows)
- TAO_AV_UDP_MCast_Flow_Handler (Flow Handler for data sent over multicast sockets)
- TAO_AV_UDP_MCast_Transport (A transport abstraction for Multicast dgram sockets. Uses the ACE_SOCK_Dgram_Mcast to send data)
- TAO_AV_UDP_Object (TAO_AV_Protocol_Object for the User Datagram Protocol (UDP))
- TAO_AV_UDP_QoS_Acceptor (No description available)
- TAO_AV_UDP_QoS_Connector (No description available)
- TAO_AV_UDP_QoS_Factory (No description available)
- TAO_AV_UDP_QoS_Flow_Factory (No description available)
- TAO_AV_UDP_QoS_Flow_Handler (No description available)
- TAO_AV_UDP_QoS_Session_Helper (Helper class to create qos sessions, activate qos handlers and set qos (For separation of concerns))
- TAO_AV_UDP_QoS_Transport (No description available)
- TAO_AV_UDP_Transport (A transport abstraction for udp sockets. Uses the ACE_SOCK_Dgram to send the data)
- TAO_Base_StreamEndPoint (No description available)
- TAO_Basic_StreamCtrl (Base class for StreamCtrl, implements basic stream start and stop functionality)
- TAO_FDev (Implementation of the AV/Streams Flow Device. A FlowConnection is used to bind FDevs for flows, much like how a StreamCtrl is used to bind MMDevices for streams)
- TAO_FlowConnection (This class currently supports only one producer and one consumer per flow)
- TAO_FlowConsumer (No description available)
- TAO_FlowEndPoint (This class is used per flow e.g video flow and an audio flow to encapsulate the transport details)
- TAO_FlowProducer (No description available)
- TAO_FlowSpec_Entry (A helper entry class in the flow spec sequence passed to bind_devs)
- TAO_Forward_FlowSpec_Entry (No description available)
- TAO_MCastConfigIf (No description available)
- TAO_MediaControl (Abstract Mediacontrol class. The following are to be handled by the specialized media control for the specific media like camera, speaker)
- TAO_MMDevice (Implements a factory to create Endpoints and VDevs)
- TAO_Negotiator (No description available)
- TAO_PropertySet (No description available)
- TAO_Reverse_FlowSpec_Entry (No description available)
- TAO_SFP_Base (No description available)
- TAO_SFP_Consumer_Object (No description available)
- TAO_SFP_Fragment_Node (No description available)
- TAO_SFP_Fragment_Table_Entry (No description available)
- TAO_SFP_Frame_State (No description available)
- TAO_SFP_Object (No description available)
- TAO_SFP_Producer_Object (No description available)
- TAO_StreamCtrl (Implementation the A/V StreamCtrl class. this class is used to control the stream. It should be subclassed by applications that want to provide more control features)
- TAO_StreamEndPoint (The Stream EndPoint. Used to implement one endpoint of a stream that implements the transport layer)
- TAO_StreamEndPoint_A (The "A" side of a streamendpoint)
- TAO_StreamEndPoint_B (The "B" side of a streamendpoint)
- TAO_Tokenizer (No description available)
- TAO_VDev (Implements the VDev interface. One of these is created per connection, and represents device-specific parameters)
- POA_AVStreams::VDev (No description available)
- AVStreams::VDev (Implements the VDev interface. One of these is created per connection, and represents device-specific parameters)