Main Page Namespace List Class Hierarchy Alphabetical List Compound List File List Namespace Members Compound Members File Members Related Pages

# TAO_Transport Class Reference

Generic definitions for the Transport class. More...

`#include <Transport.h>`

Inheritance diagram for TAO_Transport:

[legend]
Collaboration diagram for TAO_Transport:

[legend]
List of all members.

## Public Methods
| TAO_Transport (CORBA::ULong tag, TAO_ORB_Core *orb_core)
| default creator, requres the tag value be supplied. More...
virtual | ~TAO_Transport (void)
| destructor. More...
CORBA::ULong | tag (void) const
| The OMG assigns unique tags (a 32-bit unsigned number) to each protocol. More...
TAO_ORB_Core * | orb_core (void) const
| Access the ORB that owns this connection. More...
TAO_Transport_Mux_Strategy * | tms (void) const
| The role of the TAO_Transport_Mux_Strategy is described in more detail in that class' documentation. More...
TAO_Wait_Strategy * | wait_strategy (void) const
| The role of the TAO_Wait_Strategy is described in more detail in that class' documentation. More...
int | handle_output (void)
| Callback method to reactively drain the outgoing data queue. More...
virtual int | messaging_init (CORBA::Octet major, CORBA::Octet minor)=0
| Initialising the messaging object. More...
int | bidirectional_flag (void) const
| Get/Set the bidirectional flag. More...
void | bidirectional_flag (int flag)
void | provide_handle (ACE_Handle_Set &reactor_registered, TAO_EventHandlerSet &unregistered)
| Called by the cache when the cache is closing in order to fill in a handle_set in a lock-safe manner. More...
virtual int | tear_listen_point_list (TAO_InputCDR &cdr)
| Extracts the list of listen points from the <cdr> stream. The list would have the protocol specific details of the ListenPoints. More...
void | dequeue_all (void)
int | queue_is_empty (void)
int | register_handler (void)
| This method is used by the Wait_On_Reactor strategy. More...
ssize_t | send (iovec *iov, int iovcnt, size_t &bytes_transferred, const ACE_Time_Value *timeout=0)
| This method serializes on handler_lock_, guaranteeing that only thread can execute it on the same instance concurrently. More...
ssize_t | recv (char *buffer, size_t len, const ACE_Time_Value *timeout=0)
| This method serializes on handler_lock_, guaranteeing that only thread can execute it on the same instance concurrently. More...
int | id (void) const
| If not set, this will return an integer representation of the `this` pointer for the instance on which it's called. More...
void | id (int id)
| Set the identifier for this transport instance. More...
unsigned long | purging_order (void) const
| Return the order for the purging strategy. More...
void | purging_order (unsigned long value)
| Allow the purging strategy to set the order. More...
int | generate_locate_request (TAO_Target_Specification &spec, TAO_Operation_Details &opdetails, TAO_OutputCDR &output)
| This is a request for the transport object to write a LocateRequest header before it is sent out. More...
virtual int | generate_request_header (TAO_Operation_Details &opd, TAO_Target_Specification &spec, TAO_OutputCDR &msg)
| This is a request for the transport object to write a request header before it sends out the request. More...
virtual int | handle_input_i (TAO_Resume_Handle &rh, ACE_Time_Value *max_wait_time=0, int block=0)
| The ACE_Event_Handler adapter invokes this method as part of its handle_input() operation. More...
virtual int | send_request (TAO_Stub *stub, TAO_ORB_Core *orb_core, TAO_OutputCDR &stream, int is_synchronous, ACE_Time_Value *max_time_wait)=0
| Preparing the ORB to receive the reply only once the request is completely sent opens the system to some subtle race conditions: suppose the ORB is running in a multi-threaded configuration, thread A makes a request while thread B is using the Reactor to process all incoming requests. More...
virtual int | send_message (TAO_OutputCDR &stream, TAO_Stub *stub=0, int is_synchronous=1, ACE_Time_Value *max_time_wait=0)=0
| Once the ORB is prepared to receive a reply (see send_request() above), and all the arguments have been marshaled the CDR stream must be 'formatted', i.e. More...
virtual void | connection_handler_closing (void)
| Method for the connection handler to signify that it is being closed and destroyed. More...
int | recache_transport (TAO_Transport_Descriptor_Interface *desc)
| recache ourselves in the cache. More...
void | cache_map_entry (TAO_Transport_Cache_Manager::HASH_MAP_ENTRY *entry)
| Set/Get the Cache Map entry. More...
TAO_Transport_Cache_Manager::HASH_MAP_ENTRY * | cache_map_entry (void)
int | send_message_block_chain (const ACE_Message_Block *message_block, size_t &bytes_transferred, ACE_Time_Value *max_wait_time=0)
| Send a message block chain,. More...
int | send_message_i (TAO_Stub *stub, int is_synchronous, const ACE_Message_Block *message_block, ACE_Time_Value *max_wait_time)
| the twoway flag or by the current policies in the stub. More...
int | send_message_block_chain_i (const ACE_Message_Block *message_block, size_t &bytes_transferred, ACE_Time_Value *max_wait_time)
| Send a message block chain, assuming the lock is held. More...
void | purge_entry (void)
| Cache management. More...
int | make_idle (void)
| Cache management. More...
int | handle_timeout (const ACE_Time_Value &current_time, const void *act)
Control connection lifecycle
These methods are routed through the TMS object. The TMS strategies implement them correctly.
virtual int | idle_after_send (void)
| Request has been just sent, but the reply is not received. Idle the transport now. More...
virtual int | idle_after_reply (void)
| Request is sent and the reply is received. Idle the transport now. More...
virtual void | close_connection (void)
| Call the implementation method after obtaining the lock. More...
## Static Public Methods
TAO_Transport * | _duplicate (TAO_Transport *transport)
void | release (TAO_Transport *transport)
## Protected Methods
virtual ACE_Event_Handler * | event_handler_i (void)=0
| Normally a concrete TAO_Transport object has-a ACE_Event_Handler member that function as an adapter between the ACE_Reactor framework and the TAO pluggable protocol framework. More...
virtual TAO_Pluggable_Messaging * | messaging_object (void)=0
| Return the messaging object that is used to format the data that needs to be sent. More...
virtual ssize_t | send_i (iovec *iov, int iovcnt, size_t &bytes_transferred, const ACE_Time_Value *timeout=0)=0
| Often the implementation simply forwards the arguments to the underlying ACE_Svc_Handler class. More...
virtual ssize_t | recv_i (char *buffer, size_t len, const ACE_Time_Value *timeout=0)=0
virtual void | close_connection_i (void)
| Call the corresponding connection handler's <close> method. More...
virtual int | register_handler_i (void)=0
| This method is used by the Wait_On_Reactor strategy. More...
virtual void | transition_handler_state_i (void)=0
| Typically, this just sets the pointer to the associated connection handler to zero, although it could also clear out any additional resources associated with the handler association. More...
int | parse_consolidate_messages (ACE_Message_Block &bl, TAO_Resume_Handle &rh, ACE_Time_Value *time=0)
| Called by the handle_input_i (). This method is used to parse message read by the handle_input_i () call. It also decides whether the message needs consolidation before processing. More...
int | parse_incoming_messages (ACE_Message_Block &message_block)
| Method does parsing of the message if we have a fresh message in the <message_block> or just returns if we have read part of the previously stored message. More...
size_t | missing_data (ACE_Message_Block &message_block)
| Return if we have any missing data in the queue of messages or determine if we have more information left out in the presently read message to make it complete. More...
virtual int | consolidate_message (ACE_Message_Block &incoming, ssize_t missing_data, TAO_Resume_Handle &rh, ACE_Time_Value *max_wait_time)
| Consolidate the currently read message or consolidate the last message in the queue. The consolidation of the last message in the queue is done by calling consolidate_message_queue (). More...
int | consolidate_fragments (TAO_Queued_Data *qd, TAO_Resume_Handle &rh)
| Bala: Docu??? More...
int | consolidate_message_queue (ACE_Message_Block &incoming, ssize_t missing_data, TAO_Resume_Handle &rh, ACE_Time_Value *max_wait_time)
| First consolidate the message queue. If the message is still not complete, try to read from the handle again to make it complete. If these dont help put the message back in the queue and try to check the queue if we have message to process. (the thread needs to do some work anyway :-)). More...
int | consolidate_extra_messages (ACE_Message_Block &incoming, TAO_Resume_Handle &rh)
| Called by parse_consolidate_message () if we have more messages in one read. Queue up the messages and try to process one of them, atleast at the head of them. More...
int | process_parsed_messages (TAO_Queued_Data *qd, TAO_Resume_Handle &rh)
| Process the message by sending it to the higher layers of the ORB. More...
TAO_Queued_Data * | make_queued_data (ACE_Message_Block &incoming)
| Make a queued data from the <incoming> message block. More...
## Protected Attributes
CORBA::ULong | tag_
| IOP protocol tag. More...
TAO_ORB_Core * | orb_core_
| Global orbcore resource. More...
TAO_Transport_Cache_Manager::HASH_MAP_ENTRY * | cache_map_entry_
| Our entry in the cache. We dont own this. It is here for our convinience. We cannot just change things around. More...
TAO_Transport_Mux_Strategy * | tms_
| Strategy to decide whether multiple requests can be sent over the same connection or the connection is exclusive for a request. More...
TAO_Wait_Strategy * | ws_
| Strategy for waiting for the reply after sending the request. More...
int | bidirectional_flag_
| Have we sent any info on bidirectional information or have we received any info regarding making the connection served by this transport bidirectional. More...
TAO_Queued_Message * | head_
| Implement the outgoing data queue. More...
TAO_Queued_Message * | tail_
TAO_Incoming_Message_Queue | incoming_message_queue_
| Queue of the incoming messages.. More...
ACE_Time_Value | current_deadline_
| The queue will start draining no later than <queing_deadline_> *if* the deadline is. More...
long | flush_timer_id_
| The timer ID. More...
TAO_Transport_Timer | transport_timer_
| The adapter used to receive timeout callbacks from the Reactor. More...
ACE_Lock * | handler_lock_
| This is an `ACE_Lock` that gets initialized from `TAO_ORB_Core::resource_factory()->create_cached_connection_lock ()`. More...
int | id_
| This never *never* changes over the lifespan, so we don't have to worry about locking it. More...
unsigned long | purging_order_
| Used by the LRU, LFU and FIFO Connection Purging Strategies. More...
## Private Methods
int | drain_queue (void)
| As the outgoing data is drained this method is invoked to send as much of the current message as possible. More...
int | drain_queue_i (void)
| Implement drain_queue() assuming the lock is held. More...
int | queue_is_empty_i (void)
| This version assumes that the lock is already held. More...
int | drain_queue_helper (int &iovcnt, iovec iov[])
| A helper routine used in drain_queue_i(). More...
int | schedule_output_i (void)
| Schedule handle_output() callbacks. More...
int | cancel_output_i (void)
| Cancel handle_output() callbacks. More...
void | cleanup_queue (size_t byte_count)
| Exactly <byte_count> bytes have been sent, the queue must be cleaned up as potentially several messages have been completely sent out. More...
int | check_buffering_constraints_i (TAO_Stub *stub, int &must_flush)
| Copy the contents of a message block into a Queued_Message TAO_Queued_Message *copy_message_block (const ACE_Message_Block *mb); Check if the buffering constraints have been reached. More...
int | send_synchronous_message_i (const ACE_Message_Block *message_block, ACE_Time_Value *max_wait_time)
| Send a synchronous message, i.e. block until the message is on the wire. More...
int | flush_timer_pending (void) const
| Check if the flush timer is still pending. More...
void | reset_flush_timer (void)
| The flush timer expired or was explicitly cancelled, mark it as not pending. More...
int | check_event_handler_i (const char *caller)
void | report_invalid_event_handler (const char *caller)
| Print out error messages if the event handler is not valid. More...
int | process_queue_head (TAO_Resume_Handle &rh)
| Process the message that is in the head of the incoming queue. If there are more messages in the queue, this method sends a notify () to the reactor to send a next thread along. More...
| TAO_Transport (const TAO_Transport &)
| Prohibited. More...
void | operator= (const TAO_Transport &)
## Friends
class | TAO_Transport_Cache_Manager
| This class needs priviledged access to - close_connection_i(). More...
class | TAO_Block_Flushing_Strategy
| This class needs priviledged access to - queue_is_empty_i() - drain_queue_i(). More...
class | TAO_Reactive_Flushing_Strategy
| These classes need privileged access to: - schedule_output_i() - cancel_output_i(). More...
class | TAO_Leader_Follower_Flushing_Strategy

## Detailed Description

Generic definitions for the Transport class.

The transport object is created in the Service handler constructor and deleted in the Service Handler's destructor!!

The main responsability of a Transport object is to encapsulate a connection, and provide a transport independent way to send and receive data. Since TAO is heavily based on the Reactor for all if not all its I/O the Transport class is usually implemented with a helper Connection Handler that adapts the generic Transport interface to the Reactor types.

### The outgoing data path:

One of the responsibilities of the TAO_Transport class is to send out GIOP messages as efficiently as possible. In most cases messages are put out in FIFO order, the transport object will put out the message using a single system call and return control to the application. However, for oneways and AMI requests it may be more efficient (or required if the SYNC_NONE policy is in effect) to queue the messages until a large enough data set is available. Another reason to queue is that some applications cannot block for I/O, yet they want to send messages so large that a single write() operation would not be able to cope with them. In such cases we need to queue the data and use the Reactor to drain the queue.

Therefore, the Transport class may need to use a queue to temporarily hold the messages, and, in some configurations, it may need to use the Reactor to concurrently drain such queues.

### Out of order messages:

TAO provides explicit policies to send 'urgent' messages. Such messages may put at the head of the queue. However, they cannot be sent immediately because the transport may already be sending another message in a reactive fashion.

Consequently, the Transport must also know if the head of the queue has been partially sent. In that case new messages can only follow the head. Only once the head is completely sent we can start sending new messages.

### Waiting threads:

One or more threads can be blocked waiting for the connection to completely send the message. The thread should return as soon as its message has been sent, so a per-thread condition is required. This suggest that simply using a ACE_Message_Queue would not be enough: there is a significant amount of ancillary information, to keep on each message that the Message_Block class does not provide room for.

Blocking I/O is still attractive for some applications. First, my eliminating the Reactor overhead performance is improved when sending large blocks of data. Second, using the Reactor to send out data opens the door for nested upcalls, yet some applications cannot deal with the reentrancy issues in this case.

### Timeouts:

Some or all messages could have a timeout period attached to them. The timeout source could either be some high-level policy or maybe some strategy to prevent denial of service attacks. In any case the timeouts are per-message, and later messages could have shorter timeouts. In fact, some kind of scheduling (such as EDF) could be required in a few applications.

### Conclusions:

The outgoing data path consist in several components:

- A queue of pending messages
- A message currently being transmitted
- A per-transport 'send strategy' to choose between blocking on write, blocking on the reactor or blockin on leader/follower.
- A per-message 'waiting object'
- A per-message timeout

The Transport object provides a single method to send messages (send_message ()).

### The incoming data path:

One of the main responsibilities of the transport is to read and process the incoming GIOP message as quickly and efficiently as possible. There are other forces that needs to be given due consideration. They are

- Multiple threads should be able to tarverse along the same data path but should not be able to read from the same handle at the same time ie. the handle should not be shared between threads at any instant.
- Reads on the handle could give one or more messages.
- Minimise locking and copying overhead when trying to attack the above.

### Parsing messages (GIOP) & processing the message:

The messages should be checked for validity and the right information should be sent to the higher layer for processing. The process of doing a sanity check and preparing the messages for the higher layers of the ORB are done by the messaging protocol.

### Design forces and Challenges

To keep things as efficient as possible for medium sized requests, it would be good to minimise data copying and locking along the incoming path ie. from the time of reading the data from the handle to the application. We achieve this by creating a buffer on stack and reading the data from the handle into the buffer. We then pass the same data block (the buffer is encapsulated into a data block) to the higher layers of the ORB. The problems stem from the following (a) Data is bigger than the buffer that we have on stack (b) Transports like TCP do not guarentee availability of the whole chunk of data in one shot. Data could trickle in byte by byte. (c) Single read gives multiple messages

We solve the problems as follows

(a) First do a read with the buffer on stack. Query the underlying messaging object whether the message has any incomplete portion. If so, we just grow the buffer for the missing size and read the rest of the message. We free the handle and then send the message to the higher layers of the ORB for processing.

(b) If we block (ie. if we receive a EWOULDBLOCK) while trying to do the above (ie. trying to read after growing the buffer size) we put the message in a queue and return back to the reactor. The reactor would call us back when the handle becomes read ready.

(c) If we get multiple messages (possible if the client connected to the server sends oneways or AMI requests), we parse and split the messages. Every message is put in the queue. Once the messages are queued, the thread picks up one message to send to the higher layers of the ORB. Before doing that, if it finds more messages, it sends a notify to the reactor without resuming the handle. The next thread picks up a message from the queue and processes that. Once the queue is drained the last thread resumes the handle.

See Also:

http://ace.cs.wustl.edu/cvsweb/ace-latest.cgi/ACE_wrappers/TAO/docs/pluggable_protocols/index.html

## Constructor & Destructor Documentation

TAO_Transport::TAO_Transport | ( | CORBA::ULong | tag,
|  | TAO_ORB_Core * | orb_core
| ) |

| default creator, requres the tag value be supplied.

TAO_Transport::~TAO_Transport | ( | void |  | ) | `[virtual]`

| destructor.

TAO_Transport::TAO_Transport | ( | const TAO_Transport & |  | ) | `[private]`

| Prohibited.

## Member Function Documentation

TAO_Transport * TAO_Transport::_duplicate | ( | TAO_Transport * | transport | ) | `[static]`

ACE_INLINE void TAO_Transport::bidirectional_flag | ( | int | flag | ) |

ACE_INLINE int TAO_Transport::bidirectional_flag | ( | void |  | ) | const

| Get/Set the bidirectional flag.

ACE_INLINE TAO_Transport_Cache_Manager::HASH_MAP_ENTRY * TAO_Transport::cache_map_entry | ( | void |  | ) |

ACE_INLINE void TAO_Transport::cache_map_entry | ( | TAO_Transport_Cache_Manager::HASH_MAP_ENTRY * | entry | ) |

| Set/Get the Cache Map entry.

int TAO_Transport::cancel_output_i | ( | void |  | ) | `[private]`

| Cancel handle_output() callbacks.

int TAO_Transport::check_buffering_constraints_i | ( | TAO_Stub * | stub,
|  | int & | must_flush
| ) | `[private]`

| Copy the contents of a message block into a Queued_Message TAO_Queued_Message *copy_message_block (const ACE_Message_Block *mb); Check if the buffering constraints have been reached.

ACE_INLINE int TAO_Transport::check_event_handler_i | ( | const char * | caller | ) | `[private]`

| Returns: Returns -1 if not, 0 if it is.

void TAO_Transport::cleanup_queue | ( | size_t | byte_count | ) | `[private]`

| Exactly <byte_count> bytes have been sent, the queue must be cleaned up as potentially several messages have been completely sent out. It leaves on head_ the next message to send out.

void TAO_Transport::close_connection | ( | void |  | ) | `[virtual]`

| Call the implementation method after obtaining the lock.

void TAO_Transport::close_connection_i | ( | void |  | ) | `[protected, virtual]`

| Call the corresponding connection handler's <close> method.

void TAO_Transport::connection_handler_closing | ( | void |  | ) | `[virtual]`

| Method for the connection handler to signify that it is being closed and destroyed.

int TAO_Transport::consolidate_extra_messages | ( | ACE_Message_Block & | incoming,
|  | TAO_Resume_Handle & | rh
| ) | `[protected]`

| Called by parse_consolidate_message () if we have more messages in one read. Queue up the messages and try to process one of them, atleast at the head of them.

int TAO_Transport::consolidate_fragments | ( | TAO_Queued_Data * | qd,
|  | TAO_Resume_Handle & | rh
| ) | `[protected]`

| Bala: Docu??? @

int TAO_Transport::consolidate_message | ( | ACE_Message_Block & | incoming,
|  | ssize_t | missing_data,
|  | TAO_Resume_Handle & | rh,
|  | ACE_Time_Value * | max_wait_time
| ) | `[protected, virtual]`

| Consolidate the currently read message or consolidate the last message in the queue. The consolidation of the last message in the queue is done by calling consolidate_message_queue ().

int TAO_Transport::consolidate_message_queue | ( | ACE_Message_Block & | incoming,
|  | ssize_t | missing_data,
|  | TAO_Resume_Handle & | rh,
|  | ACE_Time_Value * | max_wait_time
| ) | `[protected]`

| First consolidate the message queue. If the message is still not complete, try to read from the handle again to make it complete. If these dont help put the message back in the queue and try to check the queue if we have message to process. (the thread needs to do some work anyway :-)).

void TAO_Transport::dequeue_all | ( | void |  | ) |

| Todo: : shouldn't this be automated?

int TAO_Transport::drain_queue | ( | void |  | ) | `[private]`

| As the outgoing data is drained this method is invoked to send as much of the current message as possible. Returns 0 if there is more data to send, -1 if there was an error and 1 if the message was completely sent.

int TAO_Transport::drain_queue_helper | ( | int & | iovcnt,
|  | iovec | iov[]
| ) | `[private]`

| A helper routine used in drain_queue_i().

int TAO_Transport::drain_queue_i | ( | void |  | ) | `[private]`

| Implement drain_queue() assuming the lock is held.

virtual ACE_Event_Handler* TAO_Transport::event_handler_i | ( | void |  | ) | `[protected, pure virtual]`

| Normally a concrete TAO_Transport object has-a ACE_Event_Handler member that function as an adapter between the ACE_Reactor framework and the TAO pluggable protocol framework. In all the protocols implemented so far this role is fullfilled by an instance of ACE_Svc_Handler. Todo: Since we only use a limited functionality of ACE_Svc_Handler we could probably implement a generic adapter class (TAO_Transport_Event_Handler or something), this will reduce footprint and simplify the process of implementing a pluggable protocol. Reimplemented in TAO_IIOP_Transport.

ACE_INLINE int TAO_Transport::flush_timer_pending | ( | void |  | ) | const`[private]`

| Check if the flush timer is still pending.

int TAO_Transport::generate_locate_request | ( | TAO_Target_Specification & | spec,
|  | TAO_Operation_Details & | opdetails,
|  | TAO_OutputCDR & | output
| ) |

| This is a request for the transport object to write a LocateRequest header before it is sent out.

int TAO_Transport::generate_request_header | ( | TAO_Operation_Details & | opdetails,
|  | TAO_Target_Specification & | spec,
|  | TAO_OutputCDR & | msg
| ) | `[virtual]`

| This is a request for the transport object to write a request header before it sends out the request. Reimplemented in TAO_IIOP_Transport.

int TAO_Transport::handle_input_i | ( | TAO_Resume_Handle & | rh,
|  | ACE_Time_Value * | max_wait_time = 0,
|  | int | block = 0
| ) | `[virtual]`

  | The ACE_Event_Handler adapter invokes this method as part of its handle_input() operation. Todo: : the method name is confusing! Calling it handle_input() would probably make things easier to understand and follow! Once a complete message is read the Transport class delegates on the Messaging layer to invoke the right upcall (on the server) or the TAO_Reply_Dispatcher (on the client side). Parameters:
  max_wait_time | In some cases the I/O is synchronous, e.g. a thread-per-connection server or when Wait_On_Read is enabled. In those cases a maximum read time can be specified.
  block | Is deprecated and ignored.

int TAO_Transport::handle_output | ( | void |  | ) |

| Callback method to reactively drain the outgoing data queue.

int TAO_Transport::handle_timeout | ( | const ACE_Time_Value & | current_time,
|  | const void * | act
| ) |

  | Parameters:
  current_time | The current time as reported from the Reactor
  act | The Asynchronous Completion Token. Currently it is interpreted as follows: If the ACT is the address of this->current_deadline_ the queueing timeout has expired and the queue should start flushing.
Returns: Returns 0 if there are no problems, -1 if there is an error Todo: In the future this function could be used to expire messages (oneways) that have been sitting for too long on the queue.

void TAO_Transport::id | ( | int | id | ) |

| Set the identifier for this transport instance.

int TAO_Transport::id | ( | void |  | ) | const

| If not set, this will return an integer representation of the `this` pointer for the instance on which it's called.

int TAO_Transport::idle_after_reply | ( | void |  | ) | `[virtual]`

| Request is sent and the reply is received. Idle the transport now.

int TAO_Transport::idle_after_send | ( | void |  | ) | `[virtual]`

| Request has been just sent, but the reply is not received. Idle the transport now.

int TAO_Transport::make_idle | ( | void |  | ) |

| Cache management.

TAO_Queued_Data * TAO_Transport::make_queued_data | ( | ACE_Message_Block & | incoming | ) | `[protected]`

| Make a queued data from the <incoming> message block.

virtual int TAO_Transport::messaging_init | ( | CORBA::Octet | major,
|  | CORBA::Octet | minor
| ) | `[pure virtual]`

| Initialising the messaging object. This would be used by the connector side. On the acceptor side the connection handler would take care of the messaging objects. Reimplemented in TAO_IIOP_Transport.

virtual TAO_Pluggable_Messaging* TAO_Transport::messaging_object | ( | void |  | ) | `[protected, pure virtual]`

| Return the messaging object that is used to format the data that needs to be sent. Reimplemented in TAO_IIOP_Transport.

size_t TAO_Transport::missing_data | ( | ACE_Message_Block & | incoming | ) | `[protected]`

| Return if we have any missing data in the queue of messages or determine if we have more information left out in the presently read message to make it complete.

void TAO_Transport::operator= | ( | const TAO_Transport & |  | ) | `[private]`

ACE_INLINE TAO_ORB_Core * TAO_Transport::orb_core | ( | void |  | ) | const

| Access the ORB that owns this connection.

int TAO_Transport::parse_consolidate_messages | ( | ACE_Message_Block & | block,
|  | TAO_Resume_Handle & | rh,
|  | ACE_Time_Value * | max_wait_time = 0
| ) | `[protected]`

| Called by the handle_input_i (). This method is used to parse message read by the handle_input_i () call. It also decides whether the message needs consolidation before processing.

int TAO_Transport::parse_incoming_messages | ( | ACE_Message_Block & | block | ) | `[protected]`

| Method does parsing of the message if we have a fresh message in the <message_block> or just returns if we have read part of the previously stored message.

int TAO_Transport::process_parsed_messages | ( | TAO_Queued_Data * | qd,
|  | TAO_Resume_Handle & | rh
| ) | `[protected]`

| Process the message by sending it to the higher layers of the ORB.

int TAO_Transport::process_queue_head | ( | TAO_Resume_Handle & | rh | ) | `[private]`

| Process the message that is in the head of the incoming queue. If there are more messages in the queue, this method sends a notify () to the reactor to send a next thread along.

void TAO_Transport::provide_handle | ( | ACE_Handle_Set & | reactor_registered,
|  | TAO_EventHandlerSet & | unregistered
| ) |

  | Called by the cache when the cache is closing in order to fill in a handle_set in a lock-safe manner. Parameters:
  reactor_registered | the ACE_Handle_Set into which the transport should place any handle registered with the reactor
  unregistered | the TAO_EventHandlerSet into which the transport should place any event handler that is not registered with anyone

void TAO_Transport::purge_entry | ( | void |  | ) |

| Cache management.

ACE_INLINE void TAO_Transport::purging_order | ( | unsigned long | value | ) |

| Allow the purging strategy to set the order.

ACE_INLINE unsigned long TAO_Transport::purging_order | ( | void |  | ) | const

| Return the order for the purging strategy.

int TAO_Transport::queue_is_empty | ( | void |  | ) |

| Returns: 1 if the queue is empty

int TAO_Transport::queue_is_empty_i | ( | void |  | ) | `[private]`

| This version assumes that the lock is already held. Use with care! Returns: 1 if the queue is empty

int TAO_Transport::recache_transport | ( | TAO_Transport_Descriptor_Interface * | desc | ) |

| recache ourselves in the cache.

ssize_t TAO_Transport::recv | ( | char * | buffer,
|  | size_t | len,
|  | const ACE_Time_Value * | timeout = 0
| ) |

  | This method serializes on handler_lock_, guaranteeing that only thread can execute it on the same instance concurrently. Parameters:
  buffer | ORB allocated buffer where the data should be @ The ACE_Time_Value *s is just a place holder for now. It is not clear this this is the best place to specify this. The actual timeout values will be kept in the Policies.

virtual ssize_t TAO_Transport::recv_i | ( | char * | buf,
|  | size_t | len,
|  | const ACE_Time_Value * | max_wait_time = 0
| ) | `[protected, pure virtual]`

  | Parameters:
  buffer | ORB allocated buffer where the data should be @ The ACE_Time_Value *s is just a place holder for now. It is not clear this this is the best place to specify this. The actual timeout values will be kept in the Policies.
Reimplemented in TAO_IIOP_Transport.

int TAO_Transport::register_handler | ( | void |  | ) |

| This method is used by the Wait_On_Reactor strategy. The transport must register its event handler with the ORB's Reactor. Todo: : I think this method is pretty much useless, the connections are *always* registered with the Reactor, except in thread-per-connection mode. In that case putting the connection in the Reactor would produce unpredictable results anyway.

virtual int TAO_Transport::register_handler_i | ( | void |  | ) | `[protected, pure virtual]`

| This method is used by the Wait_On_Reactor strategy. The transport must register its event handler with the ORB's Reactor. Todo: : I think this method is pretty much useless, the connections are *always* registered with the Reactor, except in thread-per-connection mode. In that case putting the connection in the Reactor would produce unpredictable results anyway. Reimplemented in TAO_IIOP_Transport.

void TAO_Transport::release | ( | TAO_Transport * | transport | ) | `[static]`

void TAO_Transport::report_invalid_event_handler | ( | const char * | caller | ) | `[private]`

| Print out error messages if the event handler is not valid.

ACE_INLINE void TAO_Transport::reset_flush_timer | ( | void |  | ) | `[private]`

| The flush timer expired or was explicitly cancelled, mark it as not pending.

int TAO_Transport::schedule_output_i | ( | void |  | ) | `[private]`

| Schedule handle_output() callbacks.

ssize_t TAO_Transport::send | ( | iovec * | iov,
|  | int | iovcnt,
|  | size_t & | bytes_transferred,
|  | const ACE_Time_Value * | timeout = 0
| ) |

  | This method serializes on handler_lock_, guaranteeing that only thread can execute it on the same instance concurrently. Often the implementation simply forwards the arguments to the underlying ACE_Svc_Handler class. Using the code factored out into ACE. Be careful with protocols that perform non-trivial transformations of the data, such as SSLIOP or protocols that compress the stream. Parameters:
  mblk | contains the data that must be sent. For each message block in the cont() chain all the data between rd_ptr() and wr_ptr() should be delivered to the remote peer.
  timeout | is the maximum time that the application is willing to wait for the data to be sent, useful in platforms that implement timed writes. The timeout value is obtained from the policies set by the application.
  bytes_transferred | should return the total number of bytes successfully transferred before the connection blocked. This is required because in some platforms and/or protocols multiple system calls may be required to send the chain of message blocks. The first few calls can work successfully, but the final one can fail or signal a flow control situation (via EAGAIN). In this case the ORB expects the function to return -1, errno to be appropriately set and this argument to return the number of bytes already on the OS I/O subsystem.
This call can also fail if the transport instance is no longer associated with a connection (e.g., the connection handler closed down). In that case, it returns -1 and sets errno to `ENOENT`.

virtual ssize_t TAO_Transport::send_i | ( | iovec * | iov,
|  | int | iovcnt,
|  | size_t & | bytes_transferred,
|  | const ACE_Time_Value * | max_wait_time = 0
| ) | `[protected, pure virtual]`

  | Often the implementation simply forwards the arguments to the underlying ACE_Svc_Handler class. Using the code factored out into ACE. Be careful with protocols that perform non-trivial transformations of the data, such as SSLIOP or protocols that compress the stream. Parameters:
  iov | contains the data that must be sent.
  iovcnt | is the number of iovec structures in the list where iov points.
  bytes_transferred | should return the total number of bytes successfully transferred before the connection blocked. This is required because in some platforms and/or protocols multiple system calls may be required to send the chain of message blocks. The first few calls can work successfully, but the final one can fail or signal a flow control situation (via EAGAIN). In this case the ORB expects the function to return -1, errno to be appropriately set and this argument to return the number of bytes already on the OS I/O subsystem.
  timeout | is the maximum time that the application is willing to wait for the data to be sent, useful in platforms that implement timed writes. The timeout value is obtained from the policies set by the application.
Reimplemented in TAO_IIOP_Transport.

virtual int TAO_Transport::send_message | ( | TAO_OutputCDR & | stream,
|  | TAO_Stub * | stub = 0,
|  | int | twoway = 1,
|  | ACE_Time_Value * | max_wait_time = 0
| ) | `[pure virtual]`

| Once the ORB is prepared to receive a reply (see send_request() above), and all the arguments have been marshaled the CDR stream must be 'formatted', i.e. the message_size field in the GIOP header can finally be set to the proper value. Todo: Another generic method, move to TAO_Transport. Reimplemented in TAO_IIOP_Transport.

int TAO_Transport::send_message_block_chain | ( | const ACE_Message_Block * | mb,
|  | size_t & | bytes_transferred,
|  | ACE_Time_Value * | max_wait_time = 0
| ) |

| Send a message block chain,.

int TAO_Transport::send_message_block_chain_i | ( | const ACE_Message_Block * | mb,
|  | size_t & | bytes_transferred,
|  | ACE_Time_Value * | max_wait_time
| ) |

| Send a message block chain, assuming the lock is held.

int TAO_Transport::send_message_i | ( | TAO_Stub * | stub,
|  | int | is_synchronous,
|  | const ACE_Message_Block * | message_block,
|  | ACE_Time_Value * | max_wait_time
| ) |

  | the twoway flag or by the current policies in the stub. Todo: This method name sucks, but send_message() was already taken by other silly methods! Parameters:
  stub | The object reference used for this operation, useful to obtain the current policies.
  is_synchronous | If set this method will block until the operation is completely written on the wire
  message_block | The CDR encapsulation of the GIOP message that must be sent. The message may consist of multiple Message Blocks chained through the cont() field.
  max_wait_time | The maximum time that the operation can block, used in the implementation of timeouts.

virtual int TAO_Transport::send_request | ( | TAO_Stub * | stub,
|  | TAO_ORB_Core * | orb_core,
|  | TAO_OutputCDR & | stream,
|  | int | two_way,
|  | ACE_Time_Value * | max_wait_time
| ) | `[pure virtual]`

| Preparing the ORB to receive the reply only once the request is completely sent opens the system to some subtle race conditions: suppose the ORB is running in a multi-threaded configuration, thread A makes a request while thread B is using the Reactor to process all incoming requests. Thread A could be implemented as follows: 1) send the request 2) setup the ORB to receive the reply 3) wait for the request but in this case thread B may receive the reply between step (1) and (2), and drop it as an invalid or unexpected message. Consequently the correct implementation is: 1) setup the ORB to receive the reply 2) send the request 3) wait for the reply The following method encapsulates this idiom. Todo: This is generic code, it should be factored out into the Transport class. Reimplemented in TAO_IIOP_Transport.

int TAO_Transport::send_synchronous_message_i | ( | const ACE_Message_Block * | mb,
|  | ACE_Time_Value * | max_wait_time
| ) | `[private]`

| Send a synchronous message, i.e. block until the message is on the wire.

ACE_INLINE CORBA::ULong TAO_Transport::tag | ( | void |  | ) | const

| The OMG assigns unique tags (a 32-bit unsigned number) to each protocol. New protocol tags can be obtained free of charge from the OMG, check the documents in corbafwd.h for more details.

int TAO_Transport::tear_listen_point_list | ( | TAO_InputCDR & | cdr | ) | `[virtual]`

| Extracts the list of listen points from the <cdr> stream. The list would have the protocol specific details of the ListenPoints. Reimplemented in TAO_IIOP_Transport.

ACE_INLINE TAO_Transport_Mux_Strategy * TAO_Transport::tms | ( | void |  | ) | const

| The role of the TAO_Transport_Mux_Strategy is described in more detail in that class' documentation. Enough is to say that the class is used to control how many threads can have pending requests over the same connection. Multiplexing multiple threads over the same connection conserves resources and is almost required for AMI, but having only one pending request per connection is more efficient and reduces the possibilities of priority inversions.

virtual void TAO_Transport::transition_handler_state_i | ( | void |  | ) | `[protected, pure virtual]`

| Typically, this just sets the pointer to the associated connection handler to zero, although it could also clear out any additional resources associated with the handler association. Reimplemented in TAO_IIOP_Transport.

ACE_INLINE TAO_Wait_Strategy * TAO_Transport::wait_strategy | ( | void |  | ) | const

| The role of the TAO_Wait_Strategy is described in more detail in that class' documentation. Enough is to say that the ORB can wait for a reply blocking on read(), using the Reactor to wait for multiple events concurrently or using the Leader/Followers protocol.

## Friends And Related Function Documentation

friend class TAO_Block_Flushing_Strategy`[friend]`

| This class needs priviledged access to - queue_is_empty_i() - drain_queue_i().

friend class TAO_Leader_Follower_Flushing_Strategy`[friend]`

friend class TAO_Reactive_Flushing_Strategy`[friend]`

| These classes need privileged access to: - schedule_output_i() - cancel_output_i().

friend class TAO_Transport_Cache_Manager`[friend]`

| This class needs priviledged access to - close_connection_i().

## Member Data Documentation

int TAO_Transport::bidirectional_flag_`[protected]`

| Have we sent any info on bidirectional information or have we received any info regarding making the connection served by this transport bidirectional. The flag is used as follows: + We dont want to send the bidirectional context info more than once on the connection. Why? Waste of marshalling and demarshalling time on the client. + On the server side -- once a client that has established the connection asks the server to use the connection both ways, we *dont* want the server to pack service info to the client. That is not allowed. We need a flag to prevent such a things from happening. The value of this flag will be 0 if the client sends info and 1 if the server receives the info.

TAO_Transport_Cache_Manager::HASH_MAP_ENTRY* TAO_Transport::cache_map_entry_`[protected]`

| Our entry in the cache. We dont own this. It is here for our convinience. We cannot just change things around.

ACE_Time_Value TAO_Transport::current_deadline_`[protected]`

| The queue will start draining no later than <queing_deadline_> *if* the deadline is.

long TAO_Transport::flush_timer_id_`[protected]`

| The timer ID.

ACE_Lock* TAO_Transport::handler_lock_`[protected]`

| This is an `ACE_Lock` that gets initialized from `TAO_ORB_Core::resource_factory()->create_cached_connection_lock ()`. This way, one can use a lock appropriate for the type of system, i.e., a null lock for single-threaded systems, and a real lock for multi-threaded systems.

TAO_Queued_Message* TAO_Transport::head_`[protected]`

| Implement the outgoing data queue.

int TAO_Transport::id_`[protected]`

| This never *never* changes over the lifespan, so we don't have to worry about locking it. HINT: Protocol-specific transports that use connection handler might choose to set this to the handle for their connection.

TAO_Incoming_Message_Queue TAO_Transport::incoming_message_queue_`[protected]`

| Queue of the incoming messages..

TAO_ORB_Core* TAO_Transport::orb_core_`[protected]`

| Global orbcore resource.

unsigned long TAO_Transport::purging_order_`[protected]`

| Used by the LRU, LFU and FIFO Connection Purging Strategies.

CORBA::ULong TAO_Transport::tag_`[protected]`

| IOP protocol tag.

TAO_Queued_Message* TAO_Transport::tail_`[protected]`

TAO_Transport_Mux_Strategy* TAO_Transport::tms_`[protected]`

| Strategy to decide whether multiple requests can be sent over the same connection or the connection is exclusive for a request.

TAO_Transport_Timer TAO_Transport::transport_timer_`[protected]`

| The adapter used to receive timeout callbacks from the Reactor.

TAO_Wait_Strategy* TAO_Transport::ws_`[protected]`

| Strategy for waiting for the reply after sending the request.

The documentation for this class was generated from the following files:

- Transport.h
- Transport.cpp
- Transport.inl