All the experiments run on a dual Pentium III @733Mhz, with 512Mb of RAM. The machine is running Linux (Debian 2.2), and we use gcc-2.95.2 to compile ACE+TAO, with static libraries and optimizations enabled.

ACE+TAO Configuration | config.h
ACE+TAO Configuration | platform_macros.GNU
CPU Information | /proc/cpuinfo
Available Memory | /proc/meminfo
OS Version | uname -a
Compiler Version | gcc -v
Library Version | /lib/libc.so.6