These pages track footprint and performance metrics for ACE+TAO. The results are collected on one of our nightly regression tests. The complete source for the tests is available as part of the ACE+TAO distribution . The hardware and software configuration used for these tests is described here. Notice, however, that the results contained here may be different from what you will obtain using a TAO release or beta kit, since the experiments are based on our current source tree.

More information about ACE+TAO footprints, and the continuing effort to reduce the library and application's code size can be found in the ACE+TAO subsetting page.

## Performance Results

ORB throughput, in requests per second, using the performance test in: `$ACE_ROOT/TAO/performance-tests/Single_Threaded_Latency`, the ORB configuration is optimized for single threaded applications using the `svc.conf` file in said directory. The test is executed over the loopback interface, using the `run_test.pl` driver script in the same directory.

## Footprint Results

Client footprint, in kilobytes, text and data segments for the test in `$ACE_ROOT/TAO/tests/ORB_init`.

Server footprint, in kilobytes, text and data segments for the test in `$ACE_ROOT/TAO/tests/ORB_init`.