Main Page Class Hierarchy Alphabetical List Compound List File List Compound Members File Members

# ACE_RMCast Compound List

Here are the classes, structs, unions and interfaces with brief descriptions:

ACE_RMCast | The RMCast namespace
ACE_RMCast::Ack | Provide feedback to the sender about messages received and sent so far
ACE_RMCast::Ack_Join | Receivers accept new members using this message
ACE_RMCast::Ack_Leave | Senders acknowledge when receivers try to leave
ACE_RMCast::Data | This is the main message sent by senders
ACE_RMCast::Join | Receivers send this message to indicate they want to join
ACE_RMCast::Leave | Receivers send this message to disconnect gracefully
ACE_RMCast::Poll |
ACE_RMCast_Ack_Worker | The retransmission module uses internal iterators, thus it needs to create helper Worker classes to process some messages
ACE_RMCast_Copy_On_Write< KEY, ITEM, COLLECTION, ITERATOR > | Implement a copy on write wrapper for a map-like collection
ACE_RMCast_Copy_On_Write_Collection< COLLECTION, ITERATOR > | A wrapper to implement reference counted collections
ACE_RMCast_Copy_On_Write_Container< COLLECTION, ITERATOR > | Base class for the Copy_On_Write collection, used to simplify the declaration of the Write_Guard
ACE_RMCast_Copy_On_Write_Read_Guard< COLLECTION, ITERATOR > | Implement a read guard for a reference counted collection
ACE_RMCast_Copy_On_Write_Write_Guard< COLLECTION, ITERATOR > | Implement the write guard for a reference counted collecion
ACE_RMCast_Fork | In some instances the messages must be sent to multiple destinations, this module is a generic component to duplicate such messages
ACE_RMCast_Fragment | Fragmentation module
ACE_RMCast_IO_UDP |
ACE_RMCast_Membership | Reliable senders of events need to know exactly how many peers are receiving the events, and how many events has each peer received so far
ACE_RMCast_Module | Reliable Multicast Module
ACE_RMCast_Module_Factory | Create Module stacks
ACE_RMCast_Partial_Message | Represent a partially received message in the ACE_RMCast_Reassembly module
ACE_RMCast_Partial_Message::Hole | Represent a missing portion of a message
ACE_RMCast_Proxy | Local representation for remote peers
ACE_RMCast_Reassembly | Reassemble multiple data fragments into a single data message
ACE_RMCast_Receiver_Module | A receiver proxy must reject invalid messages and communicate with the sender to join and leave the multicast group
ACE_RMCast_Reliable_Factory | Many applications (and even some internal components), will use a single ACE_RMCast_Module to process all the events, for example, a receiver may decide to use the same ACE_RMCast_Module to process all incoming events, instead of using one per remote sender
ACE_RMCast_Reordering | Some applications require receivers to process messages in the same order that messages are sent
ACE_RMCast_Resend_Handler | Implement an adapter to resend messages in the ACE_RMCast_Retransmission layer, but based on Reactor based timeouts
ACE_RMCast_Resend_Worker | The retransmission module uses internal iterators, thus it needs to create helper Worker classes to process some messages
ACE_RMCast_Retransmission | Reliable configurations of the RMCast framework need to store messages on the sender side to resend them if one or more clients do not receive them successfully
ACE_RMCast_Sequencer | On the sender side we must assign sequence numbers to the messages before they are put in the retransmission queue
ACE_RMCast_Singleton_Factory | Many applications (and even some internal components), will use a single ACE_RMCast_Module to process all the events, for example, a receiver may decide to use the same ACE_RMCast_Module to process all incoming events, instead of using one per remote sender
ACE_RMCast_UDP_Event_Handler | Implement an Adapter for the ACE_RMCast_IO_UDP class
ACE_RMCast_UDP_Proxy | Proxy objects are transport specific, they are responsible for storing the remote peer addressing information
ACE_RMCast_UDP_Reliable_Receiver |
ACE_RMCast_UDP_Reliable_Sender |
ACE_RMCast_Worker< KEY, ITEM > |