Main Page Class Hierarchy Alphabetical List Compound List File List Compound Members File Members Related Pages

# ACE_ATM_Connector Class Reference

Defines an active connection factory for the ACE_ATM C++ wrappers. More...

`#include <ATM_Connector.h>`

Collaboration diagram for ACE_ATM_Connector:

[legend]
List of all members.

## Public Types
typedef ACE_ATM_Addr | PEER_ADDR
typedef ACE_ATM_Stream | PEER_STREAM
## Public Methods
| ACE_ATM_Connector (void)
| Default constructor. More...
| ACE_ATM_Connector (ACE_ATM_Stream &new_stream, const ACE_ATM_Addr &remote_sap, ACE_ATM_Params params=ACE_ATM_Params(), ACE_ATM_QoS options=ACE_ATM_QoS(), ACE_Time_Value *timeout=0, const ACE_ATM_Addr &local_sap=ACE_ATM_Addr("", 0), int reuse_addr=0, int flags=0, int perms=0)
int | connect (ACE_ATM_Stream &new_stream, const ACE_ATM_Addr &remote_sap, ACE_ATM_Params params=ACE_ATM_Params(), ACE_ATM_QoS options=ACE_ATM_QoS(), ACE_Time_Value *timeout=0, const ACE_ATM_Addr &local_sap=ACE_ATM_Addr("", 0), int reuse_addr=0, int flags=0, int perms=0)
int | complete (ACE_ATM_Stream &new_stream, ACE_ATM_Addr *remote_sap, ACE_Time_Value *tv)
int | add_leaf (ACE_ATM_Stream &current_stream, const ACE_Addr &remote_sap, ACE_ATM_QoS &qos)
int | reset_new_handle (ACE_HANDLE handle)
| Resets any event associations on this handle. More...
void | dump (void) const
| Dump the state of an object. More...
## Public Attributes
| ACE_ALLOC_HOOK_DECLARE
| Declare the dynamic allocation hooks. More...
## Private Attributes
ATM_Connector | connector_

## Detailed Description

Defines an active connection factory for the ACE_ATM C++ wrappers.

## Member Typedef Documentation

typedef ACE_ATM_Addr ACE_ATM_Connector::PEER_ADDR

typedef ACE_ATM_Stream ACE_ATM_Connector::PEER_STREAM

## Constructor & Destructor Documentation

ACE_ATM_Connector::ACE_ATM_Connector | ( | void |  | ) |

| Default constructor.

ACE_INLINE ACE_ATM_Connector::ACE_ATM_Connector | ( | ACE_ATM_Stream & | new_stream,
|  | const ACE_ATM_Addr & | remote_sap,
|  | ACE_ATM_Params | params = ACE_ATM_Params(),
|  | ACE_ATM_QoS | options = ACE_ATM_QoS(),
|  | ACE_Time_Value * | timeout = 0,
|  | const ACE_ATM_Addr & | local_sap = ACE_ATM_Addr( "", 0 ),
|  | int | reuse_addr = 0,
|  | int | flags = 0,
|  | int | perms = 0
| ) |

| Actively connect and produce a <new_stream> if things go well. The <remote_sap> is the address that we are trying to connect with. The <params> are the parameters needed for either socket or XTI/ATM connections. The <timeout> is the amount of time to wait to connect. If it's 0 then we block indefinitely. If *timeout == {0, 0} then the connection is done using non-blocking mode. In this case, if the connection can't be made immediately the value of -1 is returned with <errno == EWOULDBLOCK>. If *timeout > {0, 0} then this is the maximum amount of time to wait before timing out. If the time expires before the connection is made <errno == ETIME>. The <local_sap> is the value of local address to bind to. If it's the default value of <ACE_ATM_Addr::sap_any> then the user is letting the OS do the binding. If <reuse_addr> == 1 then the <local_addr> is reused, even if it hasn't been cleanedup yet.

## Member Function Documentation

ACE_INLINE int ACE_ATM_Connector::add_leaf | ( | ACE_ATM_Stream & | current_stream,
|  | const ACE_Addr & | remote_sap,
|  | ACE_ATM_QoS & | qos
| ) |

| Actively add a leaf to the root (i.e., point-to-multipoint). The <remote_sap> is the address of the leaf that we are trying to add.

ACE_INLINE int ACE_ATM_Connector::complete | ( | ACE_ATM_Stream & | new_stream,
|  | ACE_ATM_Addr * | remote_sap,
|  | ACE_Time_Value * | tv
| ) |

| Try to complete a non-blocking connection. If connection completion is successful then <new_stream> contains the connected ACE_SOCK_Stream. If <remote_sap> is non-NULL then it will contain the address of the connected peer.

int ACE_ATM_Connector::connect | ( | ACE_ATM_Stream & | new_stream,
|  | const ACE_ATM_Addr & | remote_sap,
|  | ACE_ATM_Params | params = ACE_ATM_Params(),
|  | ACE_ATM_QoS | options = ACE_ATM_QoS(),
|  | ACE_Time_Value * | timeout = 0,
|  | const ACE_ATM_Addr & | local_sap = ACE_ATM_Addr( "", 0 ),
|  | int | reuse_addr = 0,
|  | int | flags = 0,
|  | int | perms = 0
| ) |

| Actively connect and produce a <new_stream> if things go well. The <remote_sap> is the address that we are trying to connect with. The <params> are the parameters needed for either socket or XTI/ATM connections. The <timeout> is the amount of time to wait to connect. If it's 0 then we block indefinitely. If *timeout == {0, 0} then the connection is done using non-blocking mode. In this case, if the connection can't be made immediately the value of -1 is returned with <errno == EWOULDBLOCK>. If *timeout > {0, 0} then this is the maximum amount of time to wait before timing out. If the time expires before the connection is made <errno == ETIME>. The <local_sap> is the value of local address to bind to. If it's the default value of <ACE_ATM_Addr::sap_any> then the user is letting the OS do the binding. If <reuse_addr> == 1 then the <local_addr> is reused, even if it hasn't been cleanedup yet.

void ACE_ATM_Connector::dump | ( | void |  | ) | const

| Dump the state of an object.

ACE_INLINE int ACE_ATM_Connector::reset_new_handle | ( | ACE_HANDLE | handle | ) |

| Resets any event associations on this handle.

## Member Data Documentation

ACE_ATM_Connector::ACE_ALLOC_HOOK_DECLARE

| Declare the dynamic allocation hooks.

ATM_Connector ACE_ATM_Connector::connector_`[private]`

The documentation for this class was generated from the following files:

- ATM_Connector.h
- ATM_Connector.cpp
- ATM_Connector.i