Main Page Namespace List Class Hierarchy Alphabetical List Compound List File List Namespace Members Compound Members File Members Related Pages

# IOP Namespace Reference

## Compounds
class | _tao_seq_IOP_TaggedProfile_
class | Codec
class | InvalidTypeForEncoding
class | FormatMismatch
class | TypeMismatch
class | CodecFactory
struct | Encoding
class | UnknownEncoding
struct | IOR
class | MultipleComponentProfile
struct | ServiceContext
class | ServiceContextList
struct | TaggedComponent
class | TaggedComponentList
class | TaggedComponentSeq
struct | TaggedProfile
## Typedefs
typedef Codec * | Codec_ptr
typedef TAO_Objref_Var_T< Codec > | Codec_var
typedef TAO_Objref_Out_T< Codec > | Codec_out
typedef CORBA::Short | EncodingFormat
typedef CORBA::Short_out | EncodingFormat_out
typedef TAO_Fixed_Var_T< Encoding > | Encoding_var
typedef Encoding & | Encoding_out
typedef CodecFactory * | CodecFactory_ptr
typedef TAO_Objref_Var_T< CodecFactory > | CodecFactory_var
typedef TAO_Objref_Out_T< CodecFactory > | CodecFactory_out
typedef CORBA::ULong | ProfileId
typedef CORBA::ULong_out | ProfileId_out
typedef TAO_Var_Var_T< TaggedProfile > | TaggedProfile_var
typedef TAO_Out_T< TaggedProfile, TaggedProfile_var > | TaggedProfile_out
typedef TAO_Var_Var_T< IOR > | IOR_var
typedef TAO_Out_T< IOR, IOR_var > | IOR_out
typedef CORBA::ULong | ComponentId
typedef CORBA::ULong_out | ComponentId_out
typedef TAO_Var_Var_T< TaggedComponent > | TaggedComponent_var
typedef TAO_Out_T< TaggedComponent, TaggedComponent_var > | TaggedComponent_out
typedef TAO_VarSeq_Var_T< MultipleComponentProfile, TaggedComponent > | MultipleComponentProfile_var
typedef TAO_Seq_Out_T< MultipleComponentProfile, MultipleComponentProfile_var, TaggedComponent > | MultipleComponentProfile_out
typedef TAO_VarSeq_Var_T< TaggedComponentList, TaggedComponent > | TaggedComponentList_var
typedef TAO_Seq_Out_T< TaggedComponentList, TaggedComponentList_var, TaggedComponent > | TaggedComponentList_out
typedef TAO_VarSeq_Var_T< TaggedComponentSeq, TaggedComponent > | TaggedComponentSeq_var
typedef TAO_Seq_Out_T< TaggedComponentSeq, TaggedComponentSeq_var, TaggedComponent > | TaggedComponentSeq_out
typedef CORBA::ULong | ServiceId
typedef CORBA::ULong_out | ServiceId_out
typedef TAO_Var_Var_T< ServiceContext > | ServiceContext_var
typedef TAO_Out_T< ServiceContext, ServiceContext_var > | ServiceContext_out
typedef TAO_VarSeq_Var_T< ServiceContextList, ServiceContext > | ServiceContextList_var
typedef TAO_Seq_Out_T< ServiceContextList, ServiceContextList_var, ServiceContext > | ServiceContextList_out
## Variables
::CORBA::TypeCode_ptr | _tc_Codec
::CORBA::TypeCode_ptr | _tc_EncodingFormat
::CORBA::TypeCode_ptr | _tc_Encoding
::CORBA::TypeCode_ptr | _tc_CodecFactory
const IOP::EncodingFormat | ENCODING_CDR_ENCAPS = 0
::CORBA::TypeCode_ptr | _tc_ProfileId
::CORBA::TypeCode_ptr | _tc_TaggedProfile
::CORBA::TypeCode_ptr | _tc_IOR
::CORBA::TypeCode_ptr | _tc_ComponentId
::CORBA::TypeCode_ptr | _tc_TaggedComponent
::CORBA::TypeCode_ptr | _tc_MultipleComponentProfile
::CORBA::TypeCode_ptr | _tc_TaggedComponentList
::CORBA::TypeCode_ptr | _tc_TaggedComponentSeq
::CORBA::TypeCode_ptr | _tc_ServiceId
::CORBA::TypeCode_ptr | _tc_ServiceContext
::CORBA::TypeCode_ptr | _tc_ServiceContextList
const IOP::ProfileId | TAG_INTERNET_IOP = 0U
const IOP::ProfileId | TAG_MULTIPLE_COMPONENTS = 1U
const IOP::ComponentId | TAG_ORB_TYPE = 0U
const IOP::ComponentId | TAG_CODE_SETS = 1U
const IOP::ComponentId | TAG_POLICIES = 2U
const IOP::ComponentId | TAG_ALTERNATE_IIOP_ADDRESS = 3U
const IOP::ComponentId | TAG_COMPLETE_OBJECT_KEY = 5U
const IOP::ComponentId | TAG_ENDPOINT_ID_POSITION = 6U
const IOP::ComponentId | TAG_LOCATION_POLICY = 12U
const IOP::ComponentId | TAG_DCE_STRING_BINDING = 100U
const IOP::ComponentId | TAG_DCE_BINDING_NAME = 101U
const IOP::ComponentId | TAG_DCE_NO_PIPES = 102U
const IOP::ServiceId | TransactionService = 0U
const IOP::ServiceId | CodeSets = 1U
const IOP::ServiceId | ChainBypassCheck = 2U
const IOP::ServiceId | ChainBypassInfo = 3U
const IOP::ServiceId | LogicalThreadId = 4U
const IOP::ServiceId | BI_DIR_IIOP = 5U
const IOP::ServiceId | SendingContextRunTime = 6U
const IOP::ServiceId | INVOCATION_POLICIES = 7U
const IOP::ServiceId | UnknownExceptionInfo = 9U
const IOP::ServiceId | RTCorbaPriority = 10U
const IOP::ServiceId | RTCorbaPriorityRange = 11U
const IOP::ComponentId | TAG_FT_GROUP = 27U
const IOP::ComponentId | TAG_FT_PRIMARY = 28U
const IOP::ComponentId | TAG_FT_HEARTBEAT_ENABLED = 29U
const IOP::ServiceId | FT_GROUP_VERSION = 12U
const IOP::ServiceId | FT_REQUEST = 13U
const IOP::ProfileId | TAG_UIPMC = 1413566220U
const IOP::ComponentId | TAG_GROUP = 1413566211U
const IOP::ComponentId | TAG_GROUP_IIOP = 1413566212U

## Typedef Documentation

typedef TAO_Objref_Out_T< Codec > IOP::Codec_out

typedef Codec* IOP::Codec_ptr

typedef TAO_Objref_Var_T< Codec > IOP::Codec_var

typedef TAO_Objref_Out_T< CodecFactory > IOP::CodecFactory_out

typedef CodecFactory* IOP::CodecFactory_ptr

typedef TAO_Objref_Var_T< CodecFactory > IOP::CodecFactory_var

typedef CORBA::ULong IOP::ComponentId

typedef CORBA::ULong_out IOP::ComponentId_out

typedef Encoding& IOP::Encoding_out

typedef TAO_Fixed_Var_T< Encoding > IOP::Encoding_var

typedef CORBA::Short IOP::EncodingFormat

typedef CORBA::Short_out IOP::EncodingFormat_out

typedef TAO_Out_T< IOR, IOR_var > IOP::IOR_out

typedef TAO_Var_Var_T< IOR > IOP::IOR_var

typedef TAO_Seq_Out_T< MultipleComponentProfile, MultipleComponentProfile_var, TaggedComponent > IOP::MultipleComponentProfile_out

typedef TAO_VarSeq_Var_T< MultipleComponentProfile, TaggedComponent > IOP::MultipleComponentProfile_var

typedef CORBA::ULong IOP::ProfileId

typedef CORBA::ULong_out IOP::ProfileId_out

typedef TAO_Out_T< ServiceContext, ServiceContext_var > IOP::ServiceContext_out

typedef TAO_Var_Var_T< ServiceContext > IOP::ServiceContext_var

typedef TAO_Seq_Out_T< ServiceContextList, ServiceContextList_var, ServiceContext > IOP::ServiceContextList_out

typedef TAO_VarSeq_Var_T< ServiceContextList, ServiceContext > IOP::ServiceContextList_var

typedef CORBA::ULong IOP::ServiceId

typedef CORBA::ULong_out IOP::ServiceId_out

typedef TAO_Out_T< TaggedComponent, TaggedComponent_var > IOP::TaggedComponent_out

typedef TAO_Var_Var_T< TaggedComponent > IOP::TaggedComponent_var

typedef TAO_Seq_Out_T< TaggedComponentList, TaggedComponentList_var, TaggedComponent > IOP::TaggedComponentList_out

typedef TAO_VarSeq_Var_T< TaggedComponentList, TaggedComponent > IOP::TaggedComponentList_var

typedef TAO_Seq_Out_T< TaggedComponentSeq, TaggedComponentSeq_var, TaggedComponent > IOP::TaggedComponentSeq_out

typedef TAO_VarSeq_Var_T< TaggedComponentSeq, TaggedComponent > IOP::TaggedComponentSeq_var

typedef TAO_Out_T< TaggedProfile, TaggedProfile_var > IOP::TaggedProfile_out

typedef TAO_Var_Var_T< TaggedProfile > IOP::TaggedProfile_var

## Variable Documentation

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_Codec

| Initial value:
        &_tc_TAO_tc_IOP_Codec

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_CodecFactory

| Initial value:
        &_tc_TAO_tc_IOP_CodecFactory

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_ComponentId

| Initial value:
        &_tc_TAO_tc_IOP_ComponentId

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_Encoding

| Initial value:
        &_tc_TAO_tc_IOP_Encoding

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_EncodingFormat

| Initial value:
        &_tc_TAO_tc_IOP_EncodingFormat

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_IOR

| Initial value:
        &_tc_TAO_tc_IOP_IOR

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_MultipleComponentProfile

| Initial value:
        &_tc_TAO_tc_IOP_MultipleComponentProfile

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_ProfileId

| Initial value:
        &_tc_TAO_tc_IOP_ProfileId

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_ServiceContext

| Initial value:
        &_tc_TAO_tc_IOP_ServiceContext

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_ServiceContextList

| Initial value:
        &_tc_TAO_tc_IOP_ServiceContextList

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_ServiceId

| Initial value:
        &_tc_TAO_tc_IOP_ServiceId

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_TaggedComponent

| Initial value:
        &_tc_TAO_tc_IOP_TaggedComponent

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_TaggedComponentList

| Initial value:
        &_tc_TAO_tc_IOP_TaggedComponentList

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_TaggedComponentSeq

| Initial value:
        &_tc_TAO_tc_IOP_TaggedComponentSeq

TAO_NAMESPACE_STORAGE_CLASS::CORBA::TypeCode_ptr IOP::_tc_TaggedProfile

| Initial value:
        &_tc_TAO_tc_IOP_TaggedProfile

const IOP::ServiceId IOP::BI_DIR_IIOP = 5U

const IOP::ServiceId IOP::ChainBypassCheck = 2U

const IOP::ServiceId IOP::ChainBypassInfo = 3U

const IOP::ServiceId IOP::CodeSets = 1U

const IOP::EncodingFormat IOP::ENCODING_CDR_ENCAPS = 0

const IOP::ServiceId IOP::FT_GROUP_VERSION = 12U

const IOP::ServiceId IOP::FT_REQUEST = 13U

const IOP::ServiceId IOP::INVOCATION_POLICIES = 7U

const IOP::ServiceId IOP::LogicalThreadId = 4U

const IOP::ServiceId IOP::RTCorbaPriority = 10U

const IOP::ServiceId IOP::RTCorbaPriorityRange = 11U

const IOP::ServiceId IOP::SendingContextRunTime = 6U

const IOP::ComponentId IOP::TAG_ALTERNATE_IIOP_ADDRESS = 3U

const IOP::ComponentId IOP::TAG_CODE_SETS = 1U

const IOP::ComponentId IOP::TAG_COMPLETE_OBJECT_KEY = 5U

const IOP::ComponentId IOP::TAG_DCE_BINDING_NAME = 101U

const IOP::ComponentId IOP::TAG_DCE_NO_PIPES = 102U

const IOP::ComponentId IOP::TAG_DCE_STRING_BINDING = 100U

const IOP::ComponentId IOP::TAG_ENDPOINT_ID_POSITION = 6U

const IOP::ComponentId IOP::TAG_FT_GROUP = 27U

const IOP::ComponentId IOP::TAG_FT_HEARTBEAT_ENABLED = 29U

const IOP::ComponentId IOP::TAG_FT_PRIMARY = 28U

const IOP::ComponentId IOP::TAG_GROUP = 1413566211U

const IOP::ComponentId IOP::TAG_GROUP_IIOP = 1413566212U

const IOP::ProfileId IOP::TAG_INTERNET_IOP = 0U

const IOP::ComponentId IOP::TAG_LOCATION_POLICY = 12U

const IOP::ProfileId IOP::TAG_MULTIPLE_COMPONENTS = 1U

const IOP::ComponentId IOP::TAG_ORB_TYPE = 0U

const IOP::ComponentId IOP::TAG_POLICIES = 2U

const IOP::ProfileId IOP::TAG_UIPMC = 1413566220U

const IOP::ServiceId IOP::TransactionService = 0U

const IOP::ServiceId IOP::UnknownExceptionInfo = 9U