# ASNMP Overview

The Another SNMP class library is an Object Oriented programming toolkit for using IETF standard network management protocols in the Internet. The SNMP protocol is perhaps the most ubiquitous management protocol running on most very device or application deployed in the modern network today.

ASNMP is targeted to programmers that want to write command and control (C&C) applications. C&C Applications communicate with a variety of objects:

- network devices such as ATM switches, Internet routers, LAN bridges and LAN printers
- Routing protocols such as OSPF
- database servers such as ORACLE or Informix.

  ASNMP Version 1 implements a blocking SNMP Version 1 with some Version 2c additions (Counter32, Counter64 SMI values). See SNMP Version 1 as defined in the IETF Request for Comments (RFC)

- 1155
- 1157
- 1213
- 1215

  Also see the RFC 1902 spec for new SMI datatypes such as Counter64.

  ASNMP is built using the CMU SNMP and HP SNMP++ as the base classes then modified for use in the ACE framework. About 10% of the API changed during code rework. See ASNMP/asnmp/ChangeLog for details.

  ASNMP can be used for either manager applications or agent applications. The Snmp class contains the interface for manager applications. The sagent class contains the interface for agent applications. A trivial agent that implements the mib II system group per rfc1213 is in the agents/ directory.

  ## Class Heirarchy

  ##

  #

      UdpTarget - Defines a collection of attributes needed to define a
                   communications session with an SNMP agent
                  This includes  network address, response timeout, etc.

      Snmp - A logical session between NM app and agent. Provides the
             commands get, get_next, trap. Manages transactions between app and
             server.

      Pdu  - A container object that represents an SNMP Protocol Data Unit.
             A Pdu contains a command (get,getnext,trap) Varbind List list,
             a community string.

      Vb   - Aka Varbind or Variable Binding.  A pdu can have zero,
             one or more of these. A Vb consists of an Oid to identify
             the variable and a value corresponding to  one of the SMI values.
             The oid/value binding is defined in a MIB file (RFC 1155)
             Agents hava a MIB file that defines what each variable means.
             Most agents implement MIB II as defined in RFC 1156.

      The Structure of Managment Information (SMI) datatypes
      and related types are:

      Address->IpAddress->UdpAddress as well as MAC, IPX, IPXSOCK, Netbios
      Unsigned Integer
      Gauge32
      Integer32
      Counter32
      Counter64
      TimeTicks
      OctetStr
      Oid

      Sample program
      A sample Object to get obtain an Agent's Systems' Description
      given an network address and a community string.

      class system_id {
         public:
         system_id(UdpAddress addr, OctetStr read_community_string)
           {
            UdpTarget tgt;
            Snmp snmp;
            Pdu pdu;
            Oid oid("1.3.6.1.2.1.1.1.0");
            Vb vb(oid);
            tgt.set_address(addr);
            tgt.set_read_community(read_community_string);
            pdu += vb;

            if (snmp.get(pdu, tgt) == 0) {
               pdu.get_vb(vb, 0);
               vb.get_value(desc_);
            }
            else
             desc_ = ""
           }

         int get_description(OctetStr& description) {
                description =  desc_;
                return 0;
         }

      private:
          OctetStr desc_;
      };

      Future Directions
      Here are some areas for further work

- Add OO mib parser and mib code generator
- Collapse the CMU/HP code into one set of classes.
- Add full V2c support.
- Size/Speed improvements

  # References

  - UCD SNMP
  - comp.protocols.snmp
  - University of Twente
  - SNMP FAQ
  - Java based SNMP tools from Ardent
  - IBM SNMP/CMIP research