Main Page Namespace List Class Hierarchy Alphabetical List Compound List File List Namespace Members Compound Members File Members Related Pages

# ECG_Defaults.h File Reference

This graph shows which files directly or indirectly include this file:

## Defines
#define | TAO_ECG_DEFAULT_SERVICE ECG_MCAST_TWO_WAY
#define | TAO_ECG_DEFAULT_HANDLER ECG_HANDLER_BASIC
#define | TAO_ECG_DEFAULT_ADDRESS_SERVER ECG_ADDRESS_SERVER_BASIC
#define | TAO_ECG_DEFAULT_ADDRESS_SERVER_ARG 0
#define | TAO_ECG_DEFAULT_TTL 0
#define | TAO_ECG_DEFAULT_NIC 0
#define | TAO_ECG_DEFAULT_IP_MULTICAST_LOOP 1
#define | TAO_ECG_DEFAULT_NON_BLOCKING 1
#define | TAO_ECG_DEFAULT_IIOP_CONSUMEREC_CONTROL 0
#define | TAO_ECG_DEFAULT_IIOP_CONSUMEREC_CONTROL_PERIOD 5000000
#define | TAO_ECG_DEFAULT_IIOP_CONSUMEREC_CONTROL_TIMEOUT 10000
#define | TAO_ECG_DEFAULT_IIOP_ORB_ID ""
#define | TAO_ECG_DEFAULT_IIOP_USE_TTL 1
#define | TAO_ECG_DEFAULT_IIOP_USE_CONSUMER_PROXY_MAP 1

## Detailed Description

Id:
  ECG_Defaults.h,v 1.5 2003/08/09 13:17:16 jwillemsen Exp

In this file we set the compile time defaults for the event channel multicast gateway.

Author:
  Marina Spivak (marina@atdesk.com)

## Define Documentation

#define TAO_ECG_DEFAULT_ADDRESS_SERVER ECG_ADDRESS_SERVER_BASIC

#define TAO_ECG_DEFAULT_ADDRESS_SERVER_ARG 0

#define TAO_ECG_DEFAULT_HANDLER ECG_HANDLER_BASIC

#define TAO_ECG_DEFAULT_IIOP_CONSUMEREC_CONTROL 0

#define TAO_ECG_DEFAULT_IIOP_CONSUMEREC_CONTROL_PERIOD 5000000

#define TAO_ECG_DEFAULT_IIOP_CONSUMEREC_CONTROL_TIMEOUT 10000

#define TAO_ECG_DEFAULT_IIOP_ORB_ID ""

#define TAO_ECG_DEFAULT_IIOP_USE_CONSUMER_PROXY_MAP 1

#define TAO_ECG_DEFAULT_IIOP_USE_TTL 1

#define TAO_ECG_DEFAULT_IP_MULTICAST_LOOP 1

#define TAO_ECG_DEFAULT_NIC 0

#define TAO_ECG_DEFAULT_NON_BLOCKING 1

#define TAO_ECG_DEFAULT_SERVICE ECG_MCAST_TWO_WAY

#define TAO_ECG_DEFAULT_TTL 0