// ACE version
//
//

// HOSTNAMES:
// for our tests, encip1-tango.cs.wustl.edu was the receiver hostname used for atm transfers
//                tango.cs.wustl.edu was the receiver hostname used for ethernet transfers
// substitute the proper receiver hostname for your system.

// Results:
// These examples show the result files being stored in a /results directory off
// the current path.  This can be set to whatever you like.

// ATM with 64k receiver buffers
Receiver_Host: repeat 100 server -r -s -fm -p 10002 -b 65536
Sender_Host: run_test 64 encip1-tango.cs.wustl.edu ./results/ace.atm.64 10002
	 or: client -fm -s -t -l 1048576 -n 100 -h encip1-tango.cs.wustl.edu -L ./results/ace.atm.64 -p 10002

// ATM with 8k receiver buffers
Receiver_Host: repeat 100 wrapper-new-ttcp -r -s -fm -p 10002
Sender_Host: run_test 64 encip1-tango.cs.wustl.edu ./results/ace.atm.8 10002

// ETHERNET with 64k receiver buffers
Receiver_Host: repeat 100 wrapper-new-ttcp -r -s -fm -p 10002 -b 65536
Sender_Host: run_test 64 tango.cs.wustl.edu ./results/ace.ethernet.64 10002

// ETHERNET with 8k receiver buffers
Receiver_Host: repeat 100 wrapper-new-ttcp -r -s -fm -p 10002
Sender_Host: run_test 64 tango.cs.wustl.edu ./results/ace.ethernet.8 10002
